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n 1: Identification of the Substance/Mixture and of the Company/Undertaking

Product dentifier:

Identifcation as on the label/Trade name: Zinc Oxide, Enriched Zinc Oxide.
Molecular weight: 81.39

Chemical formula: Zn0.

Synonyms: Actox 14, Actox 16, Actox 216, A13-00277, Akro-zinc bar 85, Akro-zinc bar 90, Amalox, Az0-33, A20-55, Azo:
66, 42077, Az0dox-5S, Az0doxSSTT, A20-S5TT, Az0-66TT, Azo-77TT, Cadox XX 78, Chinese White, C1. 77947, C.I
Pigment White 4, Cynku tlenek (Polish), Electox 2500, Emanay zinc oxide, EMAR, Felling zinc oxide, Flowers of zinc,
GIAP 10, Green seal-8, Hubbuck's White, Kadox 15, Kadox-25, Kadox 72, K-Zinc, Outmine, Ozide, Ozlo, Permanent
White, Philosopher's wool, Powder base 900, Protox type 166, Protox type 167, Protox type 168, Protox type 165
Protox type 267, Protox type 268, Red Seal 9, Snow White, Unichem 20, Vandem VAC, Vandem VOC, White seal-7, XX
78, XX 203, XX 601, Zinca 20, Zincite, Zincoid, Zine White, ZN-0401 E 3/16, Zn O701T.

Details of the supplier of the Safety Data Sheet
Neonest AB

Storgatan 70 Solna
SE17152

Sweden

Contact detalls:

+46.76.219.9731

24-hour Emergency Contact:
Swedish Paisans Centre
Phone: 112 - Ask for Poisons Information, 112 ~ begar Giftinformation.

Other International Contacts:
CHEMTREC 24-hour: +1.703-741-5500 (US + Worldwide)
NHS: 111 (UK)

Charite: +49 30 450 531 000 (Netherlands)

INTCF: +34 917689800 (Spain)

CapTu: 33140 05 48 48 (France)

The mixture i classified according to: Regulation EC 1272/2008 [EU-GHS/CLP]

Hazard classes/Hazard categories: Hazard statement:
Aquatic Acute (Category 1) Ha00
‘Aquatic Chronic (Category 1) a0

Label elements

Hazard pictograms:
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signal Words: Warning,

Hazard Statements:

HA00 Very toxic to aquaticlfe.

HA10 Very toxic to aquatic fife with long lasting effects

Precautionary Statements:

P273 Avoid release to the environment.

P391 Collect spilage.

PSO1 Dispose of contents/container in accordance with local and national regulations.
Other hazards: None known.

Sex

n

Composition/information on Ingredients.

Substance/Mixture: Substance.

ngredients:
TSo. | Woleaar | Concentration | Classcation
Substance name (UPAC/EC
(eAcrE) EoNo. | weight % by weight £c1272/2008
Bz | ——
Znc ovide = € sy | AquaticAcuiel Wi
povw Aquatic Chronic 11410

For explanation of abbreviations see Section 16.

Sex

n 4: Firs

id Measures

Description of first aid measur
I case of inhalation: If inhaled, remove to fresh air. f breathing becomes diffcul, call a physician. f not breathing,
give artificalrespiration.

I case of skin contact: n case of contact, immediately wash skin with soap and copious amounts of water. Consult a
physician.

In case of eye contact: In case of contact with eyes, flush with copious amounts of water for at least 15 minutes.
‘Assure adequate lushing by separating the eyelids with fingers. Cal a physician.

I case of ingestion: If swallowed, wash out mouth with water, provided person is conscious. Call a physician

Most important symptoms and effects, both acute and delay

None known.

Indication of any immediate medical attention and special treatment needed: Treat symptomatically. Show this
safety data sheet to a physician or emergency room.
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n

Fire-Fighting Measures

Extinguisher media:

Suitable extinguisher media: Use water spray, alcohol-resistant foam, dry chemical or carbon dioxide.
Unsuitable extinguishing media: None known.

Special hazards arising from the mixture: Zinc/zinc oxides.

Advice for fire-fighters: Wear self-contained breathing apparatus and protective clothing to prevent contact with skin
and eyes

Further information: Standard procedure for chemical fires. Use extinguishing measures that are appropriate to local
circumstances and the surrounding environment.

Sex

n

Accidental Release Measures.

Personal precautions, protective equipment and emergency procedures:

Personal precautions: Exercise appropriate precautions to minimize direct contact with skin or eyes and prevent
inhalation of dust.

Environmental precautions: Prevent product from entering drains. Prevent further leakage or spillage if safe to do so.
Local authorities should be advised i significant spilages cannot be contained.

Methods for containment and cleaning up:
Methods for cleaning up: Sweep up, place in a sutable closed container and hold for waste disposal. Avoid raising

dust. Ventilate area and wash spill site after materia pickup is complete.

Reference to other sections:
Treat recovered material as described i the section *Disposal considerations’

Sex

n

Handling and Storage

Precautions for safe handling:

Advice on safe handli

woid formation of dust and aerosols (further processing of solid materials may result in the.
formation of combustible dusts). Provide appropriate exhaust ventilation at places where dust may be formed. Avoid
inhalation. Avoid contact with eyes, skin and clothing. Avoid prolonged or repeated exposure,

Hygiene measures: Do not eat, drink or smoke when using this product

Conditions for safe storage, including incompatibilties:
Requirements for storage areas and containers: Keep tightly closed in a dry and well-ventilated place. Never allow.
product to getin contact with water during storage. Storage class (TRGSS10): Non-Combustible Solids.

Sex Exposure Controls/Personal Protection

Control parameter

‘Components | CAS-No. | Value | Control parameters | Basis

ZincOxide | 1314132 | TWA | 2.000000 meg/m’ | USA. ACGIH Threshold Limit Values (TLV]

Remarks: Metal fume fever
STEL [ 10.000000 mg/m’ | USA. ACGIH Threshold Limit Values (TLV)
TWA | 5000000 mg/m’ | USA NIOSH-Recommended Exposure Limits

TWA_| 5000000 mg/m’ | USA. NIOSH-Recommended Exposure Limits
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ST [ 10.000000 mg/m’ | USA.NIOSH-Recommended Exposure Limits
C | 15000000 mg/m’ | UsA. NIOSH-Recommended Exposure Limits
TWA | 5000000 mg/m’ | USA. Occupational Exposure Limits (OSHA] — Table 21

Limits for Air Contaminants
TWA | 15.000000 mg/m’ | USA. Occupational Exposure Limits (OSHA] — Table 2-1
Limits for Air Contaminants

TWA | 5000000 mg/m’ | USA. Occupational Exposure Limits (OSHA] — Table 2-1
Limits for Air Contaminants
TWA | 5000000 mg/m’ | USA. Occupational Exposure Limits (OSHA] — Table Z-1

Limits for Air Contaminants

Exposure controls:

‘Appropriate engineering controls: Safety shower and eye bath. Mechanical exhaust required.

Indi

idual protection measures, such as personal protective equipment:
Eye/face protection: Safety glasses with sde-shields conforming to EN166 Use equipment for eye protection tested
and approved under appropriate government standards such as NIOSH (US) or EN 166(EL)

Hand protection: Handle with gloves. Gloves must be inspected prior t0 use. Use proper glove removal technique
(without touching glove's outer surface) to avoid skin contact with ths product. Dispose of contaminated gloves after
use in accordance with applicable laws and good laboratory practices. Wash and dry hands.

Body protections Wear protective clothing as appropriate

Respiratory protection: For nuisance exposures use type P95 (US) or type P1 (EU EN 143) partc respiator. For
igher level protection use type OV/AG/P99 (US) or type ABEK-P2 (EU EN 143) respiator cartridges. Use respiators
and components tested and approved under appropriate government standards such as NIOSH (US) or CEN (EU).

Sex

n

Physical and Chemical Properties

Information on basic physical and chemical properties
‘Appearance (form): Sold (powder].

Colour: White.

‘Odour: Odouriess.

‘Odour threshold: No data available.

Molecular Weight: 8139

PH (concentration): No data available.

Melting point/range (*C}: No data available.

Boiling point/rane (*C): No data available.

Freezing point (‘C): No data available.

Flash point ()
Evaporation rate: No data available.

Flammabiliy (solid, gas): No data available.

Ignition temperature (‘C): No data available,

Upper/lower flammability/explosive limits: No data available.
Vapour pressure (20 °C): No data available.

Vapour densi
Relative density (25 °C): 5610 g/cm’

Water solubility (g/L) at 20 °C: No data available.

No data availabl.

No data available.
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n-Octanol/Water partition coefficient: No data available.
Auto-ignition temperature: No data available.

Decomposition temperature: No data available.

Viscosity, dynamic (mPa s): No data available.

Explosive properties: The substance or mixture i not classified as explosive.
Onidising properties: The substance or mixture is ot cassified as oxidizing.

Section 10: Stability and Reactivity

Reactivity: No dangerous reaction known under conditions of normal use.
Chemical stabilty: Stable under norma conditions.

Possibilty of hazardous reactions: No dangerous reaction known under conditions of norma use
Conditions to avoid: None known.

Incompatible materials: Strong oxidizing agents.

Hazardous decomposition products: Zinc/zinc oxides, zinc oxide fumes.

Section 11: Toxicological Information

Information on toxicological effects:
Acute Toxicity:

L, Inhalation Mouse - 2500 mg/m’

Lo Oral Mouse - 7950 me/ke.

Classification according to GHS (1272/2008/€G, CLP)
Skin corrosion/iritation:
Rabbit - mild skin iritation ~24 h
Serious eye damage/eye iritation:
Rabbit - mild eye irrtation ~24 h
Respiratory or skin sensitisation:

Not classified based on available information.
‘Germ cell mutagenicity:

Hamster — embryo - unscheduled DNA synthesis.
Hamster ~ embryo ~ morphological transformation.
Hamster — embryo —sister chromatid exchange.
Guinea pig — embryo —unscheduled DNA synthesis.
Carcinogenicity:

IARC: No component of this product present at levels greater than or equal to 0.1% is identified as  probable,
possible or confirmed human carcinogen by IARC.

ACGIH: No component of this product present at levels greater than or equal to 0.1% is identified as a carcinogen or
potentialcarcinogen by ACGIH.

NTP: No component of this product present at levels greater than or equal to 0.1% is identified as a known or
anticipated carcinogen by NTP.

OSHA: No component of this product present at levels greater than or equal to 0.1% s identified as a carcinogen or
potential carcinogen by OSHA.

Reproductive toxicity:

Not classified based on available information.

Specific target organ toxicity - single exposure (STOT)

Not classified based on available information.
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Specific target organ toxicity (STOT) - repeated exposure:
Not classiied based on available information.

Aspiration toxicity:

Not classified based on available information.

Section 12: Ecological Information

Toxicity:
Toxiciy to fish: LCso - Oncorhynchus mykiss (rainbow trout) - 1.1 me/1 - 96.0 h

Toxicityto daphnia and other aquatic invertebrates: EC,o - Daphnia magna (Water flea) - 0.098 g/ -48 h
Persistence and degradabilty: No data available.

Bioaccumulative potential:
Mobility in soil: No data available.

Results of PBTE vPVB assessment: Not relevant,

Other adverse effects: An environmental hazard cannot be excluded in the event of unprofessional handling or
disposal. Very toxic to aguatic ife

o data available.

Section 13: Disposal Considerations

‘Waste treatment methods: Offer surplus and non-recyclable solutions to a licensed disposal company.

Section 14: Transport Information

pG:
Proper Shipping Name: ENVIRONMENTALLY HAZARDOUS SUBSTANCE, SOLID, N.0.5. (Zinc oxide),
Hazard Class: 9

UN Number: 3077

Packing Group: Il

EMS No.:F-4, S

Hazard Labels:

N

1ATA:
Proper Shipping Name: ENVIRONMENTALLY HAZARDOUS SUBSTANCE, SOLID, N.05. (Zinc oxidel,
Hazard Class: 9

UN Number: 3077

Packing Group: Il

Sex

n 15: Regulatory Information

EU regulations:
Regulation (EC) No. 1005/2009 on substances that deplete the ozone layer, Annex | and Il as amended
Not listed.
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Regulation (EC) No. 850/2004 on persistent organic pollutants, Annex |
Not listed.

Regulation (EU) No. 649/2012 concerning the export and import of dangerous chemicals, Annex I, Part 1 as
amended

Not listed.

Regulation (EU) No. 649/2012 concerning the export and import of dangerous chemicals, Annex I, Part 2 as
amended

Not listed.

Regulation (EU) No. 649/2012 concerning the export and import of dangerous chemicals, Annex I, Part 3 as
amended

Not listed.

Regulation (EU) No. 648/2012 concerning the export and import of dangerous chemicals, Annex V s amended

Not listed.

Regulation (EC) No. 166/2006 Annex I Pollutant Release and Transfer Registry

Not listed.

Regulation (EC) No. 1907/2006, REACH Artcle 59(10) Candidate List as currently published by ECHA

Not listed.

Authorisations
Regulation (EC) No. 1907/2006, REACH Annex XIV Substances subject to authorization, as amended
Not listed.

Restrictions on ust
Regulation (EC) No. 1907/2006 Annex XVIl Substances sublect to restriction on marketing and use

Not regulated.

Regulation (EC) No. 1907/2006, REACH Annex XVIl Substances subject to restriction on marketing and use as
amended

Not listed.

Directive 2004/37/EC on the protection of workers from the risks related to exposure to carcinogens and mutagens
atwork

Not regulated.

Directive 92/85/EEC: on the safety and health of pregnant workers and workers who have recently given birth or
are breastfeeding.

Not regulated.

Other EU regulation:
Directive 2012/18/EU on major accident hazards involving dangerous substances

Not isted.
Directive 98/24/EC on the protection of the health and safety of workers from the risks related to chemical agents
atwork.

Always applicable.

Directive 94/33/EC on the protection of young people at work

Not listed.

Other regulations: The product is classified and labelled in accordance with EC directives or respective national laws
“This Safety Data Sheet complies with the requirements of Regulation (EC) No 1907/2006, as amended.
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SARA 302 Components: No chemicals in this material are subject to the reporting requirements of SARA Tite Il
Section 302

'SARA 313 Components: The following component i subject to reporting levels established by SARA Tile Il Section
313: Zinc oxide / CAS No. 1314-13-2/ Revision Date 2007-03.01

'SARA 311/312 Hazards: No SARA Hazards

Massachusetts Right To Know Components: Zinc oxide / CAS No. 1314-13-2 / Revision Date 2007-03-01

Pennsylvania Right To Know Components: Zinc oxide / CAS No. 1314-13-2 / Revision Date 2007-03-01

New Jersey Right To Know Components: Zinc oxide / CAS No. 1314-13-2 / Revision Date 2007-03.01

California Prop. 65 Components: This product does not contain any chemicals known to the State of California to
cause cancer, bith defects or any other reproductive harm.

National regulations: Follow national regulation for work with chemical agents

‘Chemical safety assessment: No Chemical Safety Assessment has been carried out.

Sex

n 16: Other Information

Lst of abbreviations:
ACGIH American Conference of Governmentl Industrial Hygienists

ADR European Agreement Concerning the International Carriage of Dangerous Goods by Road
ALARA As Low As Is Reasonably Achievable:

AMU Atomic Mass Unit

ANSI American National Standards Institute

BLS Basic Life Support

CAM Continuous Air Monitor

(CAs Chemical Abstracts Service (divsion of the American Chemical Society)

CEN European Committee for Standardization

CERCLA Comprehensive Environmental Respanse Compensation and Liabilty Act
CLP Classifcation, Labelling and Packaging (European Union)

CPR Controlled Products Regulations (Canada)

CWA Clean Water Act (USA)

DAC Derived Air Concentration (USA)

DOE United States Department of Energy (USA]

DOT United States Department of Transportation (USA)

DSL Domestic Substances List (Canada)

ECS0 Half Maximal Effective Concentration

EINECS European Inventory of Existing Commercial Chemical Substances

EHS Environmentally Hazardous Substance

ELINCS European List of Notifed Chemical Substances

EMS Emergency Response Procedures for Ships Carrying Dangerous Goods

EPA Environmental Protection Agency (USA)

EPCRA Emergency Planning and Community Right-To-Know Act (EPCRA) of 1986
GHs Globally Harmonized System

HMIS Hazardous Material Identification System (USA)

IARC International Agency for Research on Cancer

ATA International Air Transport Association

1BC Intermediate Bulk Containers

ICAO International Civil Aviation Organization

IDLH Immediately Dangerous to Life or Health
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IMDG International Maritime Code for Dangerous Goods
LCS0 Lethal concentration, 50 percent

LDS0 Lethal dose, 50 percent

LDLO Lethal Dose Low.

LOEC Lowest Observed-Effective Concentration

MARPOL International Convention for the Prevention of Pollution from Ships
MSHA Mine Safety and Health Administration (USA)

NCRP National Council on Radiation Protection & Measurements (USA)
NDSL Non-Domestic Substances List (Canada)

NFPA National Fire Protection Association (USA)

NIOSH National Insttute for Occupational Safety and Health (USA]

NOEC No Observed Effect Concentration

N.OS. Not Otherwise Specified

NRC Nuclear Regulatory Commission (USA)

NTP National Toxicology Program (USA)

OSHA Occupational Safety and Health Administration (USA)

PBT Persistent Bioaccumulative and Toxic Chemical

PEL Permissible Exposure Limit

PIH Poisonous by Inhalation Hazard

RCRA Resource Conservation and Recovery Act (USA)

RCT Radiation Control Technician

REACH Registration, Evaluation, Authorisation and Restriction of Chemicals (Eurape)
RID Regulations Concerning the International Transport of Dangerous Goods by Rail
RTECS Registry of Toxic Effects of Chemical Substances

SARA Superfund Amendments and Reauthorization Act (USA)

TDG Transportation of Dangerous Goods (Canada)

T Toxic by Inhalation Hazard

TLV Threshold Limit Value

TPQ Threshold Planning Quantity

TSCA Toxic Substances Control Act

TWA Time Weighted Average

UN United Nations (Number)

VOC Volatile Organic Compound

PB Very Persistent Very Bioaccumulative Chemical

WGK Wassergefahrdungskdassen (Germany: Water Hazard Classes)

WHMIS Workplace Hazardous Materials Information System

References:

Not avalable.

Fulltext of any H-statements not written out n full under Sections 2 to 15
H400 Very toxic to aquaticlfe.

HA10 Very toxic to aquatic lfe with long lasting effects.

Revision information:

None.

Training information:

Follow training instructions when handling this material

Further Information:
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‘The information provided in this Safety Data Sheet is correct to the best of our knowledge, information and belief at
the date of ts publication. The information given is designed only as a guidance for safe handiing, use, processing,
storage, transportation, disposal and release and is not to be considered a warranty or quality specification. The
information relates only to the specific material designated and may not be valid for such material used in
‘combination with any other materials or n any process, unless specified in the text.
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